SdFat

Public Member Functions | List of all members
SdCardInterface Class Referenceabstract

Abstract interface for an SD card. More...

`#include <SdCardInterface.h>`

Inheritance diagram for SdCardInterface:
[legend]
Collaboration diagram for SdCardInterface:
[legend]

## Public Member Functions
virtual bool | erase (uint32_t firstSector, uint32_t lastSector)=0
virtual uint8_t | errorCode () const =0
virtual uint32_t | errorData () const =0
virtual bool | isBusy ()=0
virtual bool | readCID (cid_t *cid)=0
virtual bool | readCSD (csd_t *csd)=0
virtual bool | readOCR (uint32_t *ocr)=0
virtual bool | readSector (uint32_t sector, uint8_t *dst)=0
virtual bool | readSectors (uint32_t sector, uint8_t *dst, size_t ns)=0
virtual uint32_t | sectorCount ()=0
virtual uint32_t | status ()
virtual bool | syncDevice ()=0
virtual uint8_t | type () const =0
virtual bool | writeData (const uint8_t *src)=0
virtual bool | writeSector (uint32_t sector, const uint8_t *src)=0
virtual bool | writeSectors (uint32_t sector, const uint8_t *src, size_t ns)=0
virtual bool | writeStart (uint32_t sector)=0
virtual bool | writeStop ()=0

## Detailed Description

Abstract interface for an SD card.

Copyright (c) 2011-2020 Bill Greiman This file is part of the SdFat library for SD memory cards.

MIT License

Permission is hereby granted, free of charge, to any person obtaining a copy of this software and associated documentation files (the "Software"), to deal in the Software without restriction, including without limitation the rights to use, copy, modify, merge, publish, distribute, sublicense, and/or sell copies of the Software, and to permit persons to whom the Software is furnished to do so, subject to the following conditions:

The above copyright notice and this permission notice shall be included in all copies or substantial portions of the Software.

THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.

## Member Function Documentation

## ◆ erase()

virtual bool SdCardInterface::erase | ( | uint32_t | firstSector,
|  | uint32_t | lastSector
| ) |  |
| pure virtual

Erase a range of sectors.

Parameters

  [in] | firstSector | The address of the first sector in the range.
  [in] | lastSector | The address of the last sector in the range.

Returns
  true for success or false for failure.

Implemented in SdioCard.

## ◆ errorCode()

virtual uint8_t SdCardInterface::errorCode | ( |  | ) | const
| pure virtual

Returns
  error code.

Implemented in SdioCard.

## ◆ errorData()

virtual uint32_t SdCardInterface::errorData | ( |  | ) | const
| pure virtual

Returns
  error data.

Implemented in SdioCard.

## ◆ isBusy()

virtual bool SdCardInterface::isBusy | ( |  | ) |
| pure virtual

Returns
  true if card is busy.

Implemented in SdioCard.

## ◆ readCID()

virtual bool SdCardInterface::readCID | ( | cid_t * | cid | ) |
| pure virtual

Read a card's CID register.

Parameters

  [out] | cid | pointer to area for returned data.

Returns
  true for success or false for failure.

Implemented in SdioCard.

## ◆ readCSD()

virtual bool SdCardInterface::readCSD | ( | csd_t * | csd | ) |
| pure virtual

Read a card's CSD register.

Parameters

  [out] | csd | pointer to area for returned data.

Returns
  true for success or false for failure.

Implemented in SdioCard.

## ◆ readOCR()

virtual bool SdCardInterface::readOCR | ( | uint32_t * | ocr | ) |
| pure virtual

Read OCR register.

Parameters

  [out] | ocr | Value of OCR register.

Returns
  true for success or false for failure.

Implemented in SdioCard.

## ◆ readSector()

virtual bool BlockDeviceInterface::readSector | ( | uint32_t | sector,
|  | uint8_t * | dst
| ) |  |
| pure virtual inherited

Read a sector.

Parameters

  [in] | sector | Logical sector to be read.
  [out] | dst | Pointer to the location that will receive the data.

Returns
  true for success or false for failure.

Implemented in SdioCard.

## ◆ readSectors()

virtual bool BlockDeviceInterface::readSectors | ( | uint32_t | sector,
|  | uint8_t * | dst,
|  | size_t | ns
| ) |  |
| pure virtual inherited

Read multiple sectors.

Parameters

  [in] | sector | Logical sector to be read.
  [in] | ns | Number of sectors to be read.
  [out] | dst | Pointer to the location that will receive the data.

Returns
  true for success or false for failure.

Implemented in SdioCard.

## ◆ sectorCount()

virtual uint32_t SdCardInterface::sectorCount | ( |  | ) |
| pure virtual

Determine the size of an SD flash memory card.

Returns
  The number of 512 byte data sectors in the card or zero if an error occurs.

Implements BlockDeviceInterface.

Implemented in SdioCard.

## ◆ status()

virtual uint32_t SdCardInterface::status | ( |  | ) |
| inline virtual

Returns
  card status.

Reimplemented in SdioCard.

## ◆ syncDevice()

virtual bool BlockDeviceInterface::syncDevice | ( |  | ) |
| pure virtual inherited

End multi-sector transfer and go to idle state.

Returns
  true for success or false for failure.

Implemented in SdioCard.

## ◆ type()

virtual uint8_t SdCardInterface::type | ( |  | ) | const
| pure virtual

Return the card type: SD V1, SD V2 or SDHC/SDXC

Returns
  0 - SD V1, 1 - SD V2, or 3 - SDHC/SDXC.

Implemented in SdioCard.

## ◆ writeData()

virtual bool SdCardInterface::writeData | ( | const uint8_t * | src | ) |
| pure virtual

Write one data sector in a multiple sector write sequence.

Parameters

  [in] | src | Pointer to the location of the data to be written.

Returns
  true for success or false for failure.

Implemented in SdioCard.

## ◆ writeSector()

virtual bool BlockDeviceInterface::writeSector | ( | uint32_t | sector,
|  | const uint8_t * | src
| ) |  |
| pure virtual inherited

Writes a sector.

Parameters

  [in] | sector | Logical sector to be written.
  [in] | src | Pointer to the location of the data to be written.

Returns
  true for success or false for failure.

Implemented in SdioCard.

## ◆ writeSectors()

virtual bool BlockDeviceInterface::writeSectors | ( | uint32_t | sector,
|  | const uint8_t * | src,
|  | size_t | ns
| ) |  |
| pure virtual inherited

Write multiple sectors.

Parameters

  [in] | sector | Logical sector to be written.
  [in] | ns | Number of sectors to be written.
  [in] | src | Pointer to the location of the data to be written.

Returns
  true for success or false for failure.

Implemented in SdioCard.

## ◆ writeStart()

virtual bool SdCardInterface::writeStart | ( | uint32_t | sector | ) |
| pure virtual

Start a write multiple sectors sequence.

Parameters

  [in] | sector | Address of first sector in sequence.

Returns
  true for success or false for failure.

Implemented in SdioCard.

## ◆ writeStop()

virtual bool SdCardInterface::writeStop | ( |  | ) |
| pure virtual

End a write multiple sectors sequence.

Returns
  true for success or false for failure.

Implemented in SdioCard.

The documentation for this class was generated from the following file:

- Arduino/libraries/SdFat/src/SdCard/SdCardInterface.h