SdFat

SdCardInterface Member List

This is the complete list of members for SdCardInterface, including all inherited members.

erase(uint32_t firstSector, uint32_t lastSector)=0 | SdCardInterface | pure virtual
errorCode() const =0 | SdCardInterface | pure virtual
errorData() const =0 | SdCardInterface | pure virtual
isBusy()=0 | SdCardInterface | pure virtual
readCID(cid_t *cid)=0 | SdCardInterface | pure virtual
readCSD(csd_t *csd)=0 | SdCardInterface | pure virtual
readOCR(uint32_t *ocr)=0 | SdCardInterface | pure virtual
readSector(uint32_t sector, uint8_t *dst)=0 | BlockDeviceInterface | pure virtual
readSectors(uint32_t sector, uint8_t *dst, size_t ns)=0 | BlockDeviceInterface | pure virtual
sectorCount()=0 | SdCardInterface | pure virtual
status() | SdCardInterface | inline virtual
syncDevice()=0 | BlockDeviceInterface | pure virtual
type() const =0 | SdCardInterface | pure virtual
writeData(const uint8_t *src)=0 | SdCardInterface | pure virtual
writeSector(uint32_t sector, const uint8_t *src)=0 | BlockDeviceInterface | pure virtual
writeSectors(uint32_t sector, const uint8_t *src, size_t ns)=0 | BlockDeviceInterface | pure virtual
writeStart(uint32_t sector)=0 | SdCardInterface | pure virtual
writeStop()=0 | SdCardInterface | pure virtual
~BlockDeviceInterface() (defined in BlockDeviceInterface) | BlockDeviceInterface | inline virtual